**Additional TSSA Requirements below**

(h) 8.6.8.15.19 Step/Skirt Performance Index is amended as follows:

1. By adding the following language **(in red type only)** to the end of requirement 8.6.8.15.19,

**8.6.8.15.19**

(f) The step/skirt performance index shall conform to the requirements in 8.6.8.3 or ASME A17.3 requirement 5.1.11 (Item 7.17). The results of the test output and graphs shall be kept in the MCP. [CAD Amendment 294.22]