Technical Standards British Columbia requires the values obtained during Category 1 & 5 Testing be recorded in the MCP Logbook.

**Ministerial Order No. M259 Appendix 2**

**9** **8.6.1.7.2** *is repealed and the following substituted:*

**8.6.1.7.2Periodic Test Record.**

A periodic test record for all periodic tests shall be kept as part of the maintenance control program record both in a logbook and electronically, to be available according to the requirements of 8.6.1.4.1 (a) (3), and including all of the following:

1. the applicable Code requirement(s) and date(s) performed;
2. the name of the person or firm performing the test;
3. all values recorded from periodic tests, including printed charts or graphs;
4. if any of the alternative test methods contained in 8.6.4.20 were performed, an indication that alternative testing was utilized for the applicable requirement.

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Code**  **Reference** | **CAT 1 Test**  **Requirements** | **Device**  **Type** | **A17.2**  **Item** |  | **Day** |  |  |  |  |  |
| **Month** |  |  |  |  |  |
| **Year** | **20\_\_** | **20\_\_** | **20\_\_** | **20\_\_** | **20\_\_** |
| **8.6.8.15.4** | Driving machine and brake torque tests. | ESC, MW | 8.4.2 | Machine #1 / Machine #2 | Torque value kN | / | / | / | / | / |
| Spring #1 Length mm | / | / | / | / | / |
| Spring #2 Length mm | / | / | / | / | / |
|  | Down stopping distance mm |  |  |  |  |  |
| **8.6.8.15.18** | Comb/ Step Impact Device. | ESC, MW | 7.7.2 | Lower Comb-Step Impact Device Readings | Vertical Middle kN |  |  |  |  |  |
| Horizontal Left kN |  |  |  |  |  |
| Horizontal Right kN |  |  |  |  |  |
| Horizontal Middle kN |  |  |  |  |  |
| Upper Comb-Step Impact Device Readings | Vertical Middle kN |  |  |  |  |  |
| Horizontal Left kN |  |  |  |  |  |
| Horizontal Right kN |  |  |  |  |  |
| Horizontal Middle kN |  |  |  |  |  |